Valve EJ has flow rate=25; tunnel leads to valve MC
Valve WC has flow rate=0; tunnels lead to valves OW, RU
Valve NP has flow rate=0; tunnels lead to valves VR, KL
Valve AA has flow rate=0; tunnels lead to valves QT, AP, EZ, AK, XV
Valve VO has flow rate=6; tunnels lead to valves KM, RF, HS, LJ, IA
Valve CB has flow rate=0; tunnels lead to valves UI, UP
Valve TE has flow rate=18; tunnel leads to valve JT
Valve CZ has flow rate=0; tunnels lead to valves UP, OW
Valve LJ has flow rate=0; tunnels lead to valves DV, VO
Valve UP has flow rate=7; tunnels lead to valves SK, CB, CZ
Valve FP has flow rate=0; tunnels lead to valves OW, RE
Valve KM has flow rate=0; tunnels lead to valves SE, VO
Valve DV has flow rate=0; tunnels lead to valves LJ, UM
Valve FL has flow rate=0; tunnels lead to valves AH, TS
Valve VR has flow rate=24; tunnels lead to valves DM, TF, NP
Valve IA has flow rate=0; tunnels lead to valves VS, VO
Valve RF has flow rate=0; tunnels lead to valves VO, JF
Valve RT has flow rate=0; tunnels lead to valves UM, SE
Valve RU has flow rate=0; tunnels lead to valves AR, WC
Valve SE has flow rate=4; tunnels lead to valves GU, KM, CX, RT
Valve MC has flow rate=0; tunnels lead to valves EJ, AR
Valve TF has flow rate=0; tunnels lead to valves AH, VR
Valve CX has flow rate=0; tunnels lead to valves SE, TO
Valve GL has flow rate=11; tunnels lead to valves UY, KL, CY
Valve GU has flow rate=0; tunnels lead to valves SE, EZ
Valve VS has flow rate=0; tunnels lead to valves XN, IA
Valve EZ has flow rate=0; tunnels lead to valves AA, GU
Valve GK has flow rate=0; tunnels lead to valves FI, HZ
Valve JT has flow rate=0; tunnels lead to valves TE, XN
Valve DM has flow rate=0; tunnels lead to valves VR, HZ
Valve AR has flow rate=16; tunnels lead to valves UI, RU, MC
Valve XN has flow rate=9; tunnels lead to valves XP, JT, VS, GT, CY
Valve CY has flow rate=0; tunnels lead to valves XN, GL
Valve QT has flow rate=0; tunnels lead to valves UM, AA
Valve KL has flow rate=0; tunnels lead to valves GL, NP
Valve SK has flow rate=0; tunnels lead to valves XV, UP
Valve OW has flow rate=12; tunnels lead to valves CZ, WC, FP
Valve AK has flow rate=0; tunnels lead to valves AA, HS
Valve XV has flow rate=0; tunnels lead to valves AA, SK
Valve GT has flow rate=0; tunnels lead to valves XN, UM
Valve FI has flow rate=0; tunnels lead to valves JF, GK
Valve UY has flow rate=0; tunnels lead to valves JF, GL
Valve UM has flow rate=5; tunnels lead to valves DV, GT, RT, QT
Valve IQ has flow rate=0; tunnels lead to valves HZ, AH
Valve JF has flow rate=10; tunnels lead to valves RF, FI, UY, RE, TS
Valve TS has flow rate=0; tunnels lead to valves JF, FL
Valve AH has flow rate=23; tunnels lead to valves IQ, FL, TF
Valve HS has flow rate=0; tunnels lead to valves AK, VO
Valve HZ has flow rate=20; tunnels lead to valves IQ, DM, GK
Valve TO has flow rate=15; tunnel leads to valve CX
Valve XP has flow rate=0; tunnels lead to valves AP, XN
Valve AP has flow rate=0; tunnels lead to valves XP, AA
Valve RE has flow rate=0; tunnels lead to valves JF, FP
Valve UI has flow rate=0; tunnels lead to valves AR, CB
